**LAESA DEPLOYMENT, DR**

**10 Megawatt Wartsila Generator**

**Engine-8 Fuel Efficiency Data Analysis**

**8/13/2012**

(Note: IR canister was installed on 11/12/2011 and bypassed on 4/1)

**IR bypassed**

**on 4/1/2012**

**IR installed on 11/12/2011**

**with-IR on**

**Specific Fuel Consumption**

**(g/kWh)**

**Baseline**

**Baseline**

with-IR average

11/12 - 3/31/12

**207.0** g/kWh

Baseline average

8/12 - 11/11

**209.5** g/kWh

**Testing Date (weekly data)**